[OPTIONS]
bitmap_file=Skin.bmp
skin_file=Skin.via
wave_file=ST.WAV
icon_file=AudioDeck.ico
multi_language_file=String.via
ApplicationTitle=VIA HD Audio Deck
version=4.0 a

;===================
;= 1.True or False =
;===================
Initial_and_Exit=0
Show_TrayIcon=1
Show_TrayIcon_Option=1
Show_Welcome=1
Show_SPDIF_In_JackPage=1
Draw_RCA_CD_IN=0
Draw_RCA_SPDIF=0
bPlugIn_Mute_On=1
Show_Panel_Title=1
Show_FullRange_Speaker_Option=1
Enable_Smart51=0
ShowRecordingMasterMute=0
SimpleMode=1
Show_Plugged_Message=1

;==============================
;= 2.First time start setting =
;==============================
;
; Volume value range : 0 ~ 65535
;
WriteKeysToRegistryOK=0
First_Time_Start=1
First_Time_StartSpeaker2=1
First_Time_StartHP=1

Preset_Speaker=0
Speaker_Volume=65535
Speaker_Mute=0

Preset_Headphone=0
Headphone_Volume=65535
Headphone_Mute=0

Preset_SPDIF_OUT=0
SPDIF_OUT_Volume=65535
SPDIF_OUT_Mute=0

Preset_Mic=0
Mic_Volume=65535
Mic_Mute=0

Preset_Line_In=0
Line_In_Volume=65535
Line_In_Mute=0

Preset_SPDIF_IN=0
SPDIF_IN_Volume=65535
SPDIF_IN_Mute=0

Preset_FrontMic=0
FrontMic_Volume=65535
FrontMic_Mute=0

Preset_FrontMic2=0
FrontMic2_Volume=65535
FrontMic2_Mute=0

Preset_Stereo_Mix=0
Stereo_Mix_Volume=65535
Stereo_Mix_Mute=0

Preset_CDAudio=0
CDAudio_Volume=65535
CDAudio_Mute=0

Preset_RCA=0
RCA_Volume=65535
RCA_Mute=0

;====================
;= 3.Default device =
;====================
;
;Speaker   : 0
;Headphone : 1
;SPDIF_Out : 2
;Microphone: 3
;Stereo_Mix: 4
;Line_In   : 5
;SPDIF_In  : 6
;FrontMic  : 7
;CDAudio   : 8
;RCA       : 9
;FrontMic2 : 10
;
Default_Playback_Num = 3
Default_Playback0  = 0
Default_Playback1  = 1
Default_Playback2  = 2

Default_Recording_Num = 8
Default_Recording0 = 7
Default_Recording1 = 3
Default_Recording2 = 5
Default_Recording3 = 6
Default_Recording4 = 4
Default_Recording5 = 8
Default_Recording6 = 9
Default_Recording7 = 10

JackPluggedStatus=8

;=============
;= 4.AA Path =
;=============
;
; 1. If "AA_Path_Enable"=0, it will disable AA_Microphone, AA_LineIn, and AA_Front. But AA_PCBeep and AA_CDAudio are still work.
; 2. If "AA_PCBeep_Enable"=0, the AA_CDAudio will be disabled.
;
Show_AA_Path_Option=1
AA_Path_Enable=1

AA_PCBeep_Enable=0
AA_PCBeep_LeftVolume=65535
AA_PCBeep_RightVolume=65535
AA_PCBeep_Mute=0
AA_PCBeep_Sync=1
AA_PCBeep_MaxVolume=32768

AA_CDAudio_Enable=0
AA_CDAudio_LeftVolume=65535
AA_CDAudio_RightVolume=65535
AA_CDAudio_Mute=0
AA_CDAudio_Sync=1

AA_Microphone_Enable=0
AA_Microphone_LeftVolume=65535
AA_Microphone_RightVolume=65535
AA_Microphone_Mute=0
AA_Microphone_Sync=1

AA_LineIn_Enable=0
AA_LineIn_LeftVolume=65535
AA_LineIn_RightVolume=65535
AA_LineIn_Mute=0
AA_LineIn_Sync=1

AA_FrontMic_Enable=0
AA_FrontMic_LeftVolume=65535
AA_FrontMic_RightVolume=65535
AA_FrontMic_Mute=0
AA_FrontMic_Sync=1

;==========================
;= 5.Jack Function Status =
;==========================
VIA_PW0_BackSurrOut=0
VIA_PW1_Mic12=1
VIA_PW2_LineIn=2
VIA_PW3_FrontOut=3
VIA_PW4_HP=4
VIA_PW5_FrontMic=5
VIA_PW6_CenterLFE=6
VIA_PW7_SideSurrOut=7
VIA_PW8_CDIn=8
VIA_PW4_FrontMic2=0

;=======================
;= 6.Volume Sync State =
;=======================
;
;Speaker   : 0
;Headphone : 1
;SPDIF_Out : 2
;Microphone: 3
;Stereo_Mix: 4
;Line_In   : 5
;SPDIF_In  : 6
;FrontMic  : 7
;CDAudio   : 8
;RCA       : 9
;FrontMic2 : 10
;
Sync_0=1
Sync_0_0=1
Sync_0_1=1
Sync_0_2=1
Sync_0_3=1
Sync_1_0=1
Sync_2_0=1
Sync_3_0=1
Sync_3_1=1
Sync_4_0=1
Sync_5_0=1
Sync_5_1=1
Sync_6_0=1
Sync_7_0=1
Sync_7_1=1
Sync_8_0=1
Sync_8_1=1
Sync_9_0=1
Sync_10_0=1

;=====================
;= 7.Jack Page Style =
;=====================
Arrow_Head_On=0
Jack_Plugged_Icon_On=0
Fade_In_Out_On=1

;=================
;= 8.Jack Detect =
;=================
Show_JackDetect_Option=1
Enable_JackDetect=1
Auto_Pop_Dialog=0
Manual_Pop_Dialog=1
Show_Auto_Pop_Dialog_Option=1

;==============
;= 9.Settings =
;==============
Multi_Language=0

;======================
;= 10.Jacks' Position =
;======================
;
; position:
; ---------
; | 1 2 3 |
; | 4 5 6 |
; | 7 8 9 |
; ---------   0 denote not show.
;
; color:
; Black  : 1
; Grey   : 2
; Blue   : 3
; Green  : 4
; Red    : 5
; Orange : 6
; Yellow : 7
; Purple : 8
; Pink   : 9
; White  : 14
; 
; Back_1=xy
; x = position, y = color
;
Back_1=13
Back_2=44
Back_3=79
Back_4=26
Back_5=51
Back_6=82

Front_1=19
Front_2=24
Front_3=43

DonotCarePingConfig=0

;====================
;=  11.Information  =
;====================
URL=http://www.viatech.com

;====================
;= 12.Sound Effects =
;====================
;
; EnvironmentModeling_Index =
; 0  : Club
; 1  : Auditorium
; 2  : Bathroom
; 3  : Church
; 4  : Concert Hall
; 5  : Forest
; 6  : Living Room
; 7  : Mountains
; 8  : Quarry
; 9  : Stadium
; 10 : Theater
; 11 : Underwater
; --------------------------------
; BassManagement_Frequency = x
; 			==> ( 50 + 25 * x ) KHz
; 0 <= x <= 22
; --------------------------------
; BassManagement_BassBoost =
; 0  : None
; 1  : 3 db
; 2  : 6 db
; 3  : 9 db
; 4  : 12 db
; --------------------------------
; Equalizer_XXX = x
; 0 <= x <= 40
;---------------------------------
; RoomCorrection_0 = x : Front Left
; RoomCorrection_1 = x : Front Right
; RoomCorrection_2 = x : Center
; RoomCorrection_3 = x : LFE
; RoomCorrection_4 = x : Side Left 
; RoomCorrection_5 = x : Side Right
; RoomCorrection_6 = x : Back Left
; RoomCorrection_7 = x : Back Right
; 5 <= x <= 40
;

bEnhancement_On=1
bCenterLFE_Swap_On=0
bExpander_On=0
bLoudnessEqualization_On=0

[DevSpeaker]
bEnvironmentModeling_On=0
EnvironmentModeling_Index=0

bBassManagement_On=0
BassManagement_Frequency=0
BassManagement_BassBoost=0

bEqualizer_On=0
Equalizer_60  =20
Equalizer_170 =20
Equalizer_310 =20
Equalizer_600 =20
Equalizer_1k  =20
Equalizer_3k  =20
Equalizer_6k  =20
Equalizer_12k =20
Equalizer_14k =20
Equalizer_16k =20

bRoomCorrection_On=0
bRoomCorrection_Sync_On=0
RoomCorrection_0=23
RoomCorrection_1=23
RoomCorrection_2=23
RoomCorrection_3=23
RoomCorrection_4=23
RoomCorrection_5=23
RoomCorrection_6=23
RoomCorrection_7=23

;========================
;= 97.S3 EQ custom
;=======================
;
; EQ_Custom_1_name=Name
; EQ_Custom_1_X=
;
[EQ_Custom_DevSpeaker]
EQ_Custom_num=0

[DevHeadphone]
bEnvironmentModeling_On=0
EnvironmentModeling_Index=0

bBassManagement_On=0
BassManagement_Frequency=0
BassManagement_BassBoost=0

bEqualizer_On=0
Equalizer_60  =20
Equalizer_170 =20
Equalizer_310 =20
Equalizer_600 =20
Equalizer_1k  =20
Equalizer_3k  =20
Equalizer_6k  =20
Equalizer_12k =20
Equalizer_14k =20
Equalizer_16k =20

bRoomCorrection_On=0
bRoomCorrection_Sync_On=0
RoomCorrection_0=23
RoomCorrection_1=23
RoomCorrection_2=23
RoomCorrection_3=23
RoomCorrection_4=23
RoomCorrection_5=23
RoomCorrection_6=23
RoomCorrection_7=23

;========================
;= 97.S3 EQ custom
;=======================

[EQ_Custom_DevHeadphone]
EQ_Custom_num=0

;========================
;= 98.S3 Return Command =
;=======================
;
;EX:
;command_num=2
;command_1=00000001
;command_2=00000002
;

[S3_RETURN]
command_num=0

;======================
;= 99.Initial Command =
;======================
;
;EX:
;command_num=2
;command_1=00000001
;command_2=00000002
;

[INITIAL]
command_num=0

;====================
;= 100.Jack Command =
;====================
;
;EX:
;JACK_PLUGIN_command_num=2
;JACK_PLUGIN_1=00000001
;JACK_PLUGIN_2=00000002
;
[BackSurrOut]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[Mic12]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[LineIn]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[LineOut]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[HeadPhoneOut]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[FrontMic]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[CenterLFE]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[SideSurrOut]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0

[FrontMic2]
JACK_PLUGIN_command_num=0
JACK_PULLOUT_command_num=0
